(kicad_symbol_lib
	(version 20251024)
	(generator "kicad_symbol_editor")
	(generator_version "10.0")
	(symbol "XIAO_ESP32S3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(duplicate_pin_numbers_are_jumpers no)
		(property "Reference" "MOD1"
			(at -2.54 -11.43 0)
			(show_name no)
			(do_not_autoplace no)
		)
		(property "Value" "ESP32S3"
			(at -3.556 1.778 0)
			(show_name no)
			(do_not_autoplace no)
		)
		(property "Footprint" "RF_Module:Heltec_HT-CT62"
			(at 0 -30.48 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
		)
		(property "Datasheet" "https://resource.heltec.cn/download/HT-CT62/HT-CT62(Rev1.1).pdf"
			(at 1.016 -35.306 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
		)
		(property "Description" "LoRa/LoRaWAN node module with ESP32-C3 and SX1262"
			(at 0.254 -33.02 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
		)
		(property "ki_keywords" "LoRa WiFi ESP32 SX1262"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
		)
		(property "ki_fp_filters" "*HT?CT62*"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
		)
		(symbol "XIAO_ESP32S3_1_1"
			(pin bidirectional line
				(at -6.35 -16.51 90)
				(length 2.54)
				(name "Ant")
				(number "")
			)
			(pin bidirectional line
				(at 0 17.78 270)
				(length 2.54)
				(name "USB")
				(number "")
			)
			(pin bidirectional line
				(at -17.78 11.43 0)
				(length 2.54)
				(name "GPIO1")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "GPIO2")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 3.81 0)
				(length 2.54)
				(name "GPIO3")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "GPIO4")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -3.81 0)
				(length 2.54)
				(name "GPIO5")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "GPIO6")
				(number "6")
			)
			(pin input line
				(at -17.78 -11.43 0)
				(length 2.54)
				(name "GPIO43")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 11.43 180)
				(length 2.54)
				(name "5V")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "GPIO9")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -3.81 180)
				(length 2.54)
				(name "GPIO8")
				(number "12")
			)
			(pin passive line
				(at 0 -16.51 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "GPIO7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -11.43 180)
				(length 2.54)
				(name "GPIO44")
				(number "14")
			)
			(pin passive line
				(at 0 -16.51 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
)
