(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "GC1 Geiger Counter / GNSS Interface")
		(date "2026-09-07")
		(rev "D")
	)
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.2104)
				(material "7628")
				(epsilon_r 4.4)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0152)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.065)
				(material "FR4")
				(epsilon_r 4.6)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0152)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.2104)
				(material "7628")
				(epsilon_r 4.4)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "ENIG")
			(dielectric_constraints yes)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 74.3 25.5)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RA2"
			(at 0 -1.83 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.5M / 200V"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/GM_ANODE_CHAIN_1")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/GM_ANODE_CHAIN_2")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 58.8 52)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "Q1"
			(at 0 -4.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PBHV8560Z"
			(at 0 4.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/Q1_BASE")
		)
		(pad "2" smd roundrect
			(at -3.15 0)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/SW")
		)
		(pad "2" smd roundrect
			(at 3.15 0)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/SW")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0402_1005Metric"
		(layer "F.Cu")
		(at 38.5 29.3)
		(descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf)")
		(tags "inductor")
		(property "Reference" "L2"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "27nH"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/RF_ANT")
		)
		(pad "2" smd roundrect
			(at 0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/ACTIVE_ANT_BIAS_R")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "GC1_RevD:SBM21_Interchangeable"
		(layer "F.Cu")
		(at 65 24.2)
		(property "Reference" "MC2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keystone 6049 anode socket"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 2.2 2.2)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/TUBE_RIGHT")
		)
		(pad "1" thru_hole circle
			(at 0 -2.54)
			(size 2.2 2.2)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/TUBE_RIGHT")
		)
		(pad "1" thru_hole circle
			(at 0 2.54)
			(size 2.2 2.2)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/TUBE_RIGHT")
		)
		(pad "1" thru_hole circle
			(at 2.54 0)
			(size 2.2 2.2)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/TUBE_RIGHT")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 82.5 23.5)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "H2"
			(at 0 -3.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "H2"
			(at 0 3.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "mounting_hardware/mounting_hole"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "GC1_RevD:C_1210_TDK_CGA6M"
		(layer "F.Cu")
		(at 74.5 56.5)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -2.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7nF 1kV"
			(at 0 2.3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net "/HV_PLUS")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 79 44)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 48 31)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RK1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GM_CATHODE")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 24.5 34 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RPU1"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GNSS_I2C_SDA")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "GC1_RevD:SBM21_ASSEMBLY"
		(layer "F.Cu")
		(at 53.945 24.2)
		(property "Reference" "V1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SBM-21 GM tube"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 79 47)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.85 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net "/3V3")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 82.5 60.5)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "H3"
			(at 0 -3.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "H3"
			(at 0 3.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "mounting_hardware/mounting_hole"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "GC1_RevD:C_1210_TDK_CGA6M"
		(layer "F.Cu")
		(at 62.5 59 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -2.3 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7nF 1kV"
			(at 0 2.3 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net "/SW")
		)
		(pad "2" smd roundrect
			(at 1.65 0 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net "/PUMP")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 44 61)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HOST_UART_TX"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/HOST_UART_TX")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 48 47)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RH1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GPIO_GM_COUNT")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GM_PULSE")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "GC1_RevD:TPD1E0B04_DPY0002A"
		(layer "F.Cu")
		(at 38 31.7)
		(descr "Diode SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf)")
		(tags "diode")
		(property "Reference" "ESD1"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TPD1E0B04"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.35 0)
			(size 0.3 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(pad "2" smd roundrect
			(at 0.35 0)
			(size 0.3 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/RF_ANT")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 49 37)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GM_PULSE"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/GM_PULSE")
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 69 61.5 180)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D2"
			(at 0 -2.5 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "US1M"
			(at 0 2.6 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 180)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net "/HV_PLUS")
		)
		(pad "2" smd roundrect
			(at 2 0 180)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net "/PUMP")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:U.FL_Hirose_U.FL-R-SMT-1_Vertical"
		(layer "F.Cu")
		(at 41 34.5)
		(descr "Hirose U.FL Coaxial (https://www.hirose.com/en/product/document?clcode=CL0331-0472-2-01&productname=U.FL-R-SMT-1(01)&series=U.FL&documenttype=2DDrawing&lang=en&documentid=0000940668)")
		(tags "Hirose U.FL Coaxial")
		(property "Reference" "J1"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "U.FL"
			(at 0 3.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.525 0)
			(size 1.05 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/RF_ANT")
		)
		(pad "2" smd roundrect
			(at 0 -1.475)
			(size 2.2 1.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2380952381)
			(net "/GND")
		)
		(pad "2" smd roundrect
			(at 0 1.475)
			(size 2.2 1.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2380952381)
			(net "/GND")
		)
		(zone
			(layer "F.Cu")
			(name "top_keepout")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 42.1 33.55) (xy 40.01 33.55) (xy 40.01 35.45) (xy 42.1 35.45)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 41 30)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RANT"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10R"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/ACTIVE_ANT_BIAS_R")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/ACTIVE_ANT_BIAS")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 26.8 34 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RPU2"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GNSS_I2C_SCL")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 74.5 62)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HV_PLUS"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/HV_PLUS")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 77 32)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RF1"
			(at 0 -1.83 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "7.5M / 200V"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/HV_FB_1")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/HV_PLUS")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 48 34)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RS1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GM_PULSE")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 58 38.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RFB1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "68k 1%"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/HV_SENSE")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 57 36)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HV_SENSE"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/HV_SENSE")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 31 59)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP14"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HOST_UART_RX"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/HOST_UART_RX")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 74.3 21.5)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RA1"
			(at 0 -1.83 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.5M / 200V"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/GM_ANODE")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/GM_ANODE_CHAIN_1")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 70.1 28.7)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GM_ANODE"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/GM_ANODE")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 23 30.7 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.43 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1uF"
			(at 0 1.43 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 62 36)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RF4"
			(at 0 -1.83 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "7.5M / 200V"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/HV_SENSE")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/HV_FB_3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 45 34)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "47pF C0G"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GM_CATHODE")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GM_PULSE")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 23 28.2 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.43 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.43 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 48 60.5)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "H1"
			(at 0 -3.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "H1"
			(at 0 3.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "mounting_hardware/mounting_hole"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 46 50)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GPIO_GM_COUNT"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/GPIO_GM_COUNT")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 26 59)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP12"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3V3"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/3V3")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 22.5 59)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP11"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/GND")
		)
		(embedded_fonts no)
	)
	(footprint "GC1_RevD:SBM21_Interchangeable"
		(layer "F.Cu")
		(at 45.5 24.2)
		(property "Reference" "MC1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Littelfuse 01000058Z body clip"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 2.2 2.2)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/TUBE_LEFT")
		)
		(pad "1" thru_hole circle
			(at 0 -2.54)
			(size 2.2 2.2)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/TUBE_LEFT")
		)
		(pad "1" thru_hole circle
			(at 0 2.54)
			(size 2.2 2.2)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/TUBE_LEFT")
		)
		(pad "1" thru_hole circle
			(at 2.54 0)
			(size 2.2 2.2)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/TUBE_LEFT")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 51.8 30)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GM_CATHODE"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/GM_CATHODE")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 51.5 34)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D3"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BAT54S"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/3V3")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GM_PULSE")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 67 32)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RF3"
			(at 0 -1.83 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "7.5M / 200V"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/HV_FB_3")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/HV_FB_2")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 44.5 58)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100R"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/HOST_UART_TX_RAW")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/HOST_UART_TX")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 33 34)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP10"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GNSS_I2C_SCL"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/GNSS_I2C_SCL")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 52 48.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RB1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100R"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GPIO_HV_PWM")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/Q1_BASE")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 42 55.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100R"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/HOST_UART_RX")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/HOST_UART_RX_RAW")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 50.5 52.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RBE1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/Q1_BASE")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 44 40.7)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP17"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ACTIVE_ANT_BIAS"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/ACTIVE_ANT_BIAS")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 29 34)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GNSS_I2C_SDA"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/GNSS_I2C_SDA")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 54 38)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "180k 1%"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/3V3")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/THRESH")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 72 32)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RF2"
			(at 0 -1.83 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "7.5M / 200V"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/HV_FB_2")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/HV_FB_1")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 54 59.8 90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D1"
			(at 0 -2.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "US1M"
			(at 0 2.6 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net "/PUMP")
		)
		(pad "2" smd roundrect
			(at 2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 76 29.5)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "RA3"
			(at 0 -1.83 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.5M / 200V"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/GM_ANODE_CHAIN_2")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net "/HV_PLUS")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 51 43.5)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U2"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TLV3201DBV"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GPIO_GM_COUNT")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GM_PULSE")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/THRESH")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/3V3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 24 55.8)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/HV_SENSE")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 28.5 59)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP13"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "VBUS"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/VBUS")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 67 55)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/SW")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 54 40)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "33k 1%"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/THRESH")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 50 55.5)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP16"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/GND")
		)
		(embedded_fonts no)
	)
	(footprint "RF_GPS:ublox_MAX"
		(layer "F.Cu")
		(at 31 26)
		(descr "ublox MAX 6/7/8, (https://www.u-blox.com/sites/default/files/MAX-8-M8-FW3_HardwareIntegrationManual_%28UBX-15030059%29.pdf)")
		(tags "GPS ublox MAX 6/7/8")
		(property "Reference" "U1"
			(at 0 -6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MAX-M10S"
			(at 0 6.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.75 -4.4)
			(size 1.8 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(pad "2" smd roundrect
			(at -4.75 -3.3)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "3" smd roundrect
			(at -4.75 -2.2)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "4" smd roundrect
			(at -4.75 -1.1)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "5" smd roundrect
			(at -4.75 0)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "6" smd roundrect
			(at -4.75 1.1)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "7" smd roundrect
			(at -4.75 2.2)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/3V3")
		)
		(pad "8" smd roundrect
			(at -4.75 3.3)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/3V3")
		)
		(pad "9" smd roundrect
			(at -4.75 4.4)
			(size 1.8 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "10" smd roundrect
			(at 4.75 4.4)
			(size 1.8 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(pad "11" smd roundrect
			(at 4.75 3.3)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/RF_ANT")
		)
		(pad "12" smd roundrect
			(at 4.75 2.2)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(pad "13" smd roundrect
			(at 4.75 1.1)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "14" smd roundrect
			(at 4.75 0)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/ACTIVE_ANT_BIAS")
		)
		(pad "15" smd roundrect
			(at 4.75 -1.1)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "16" smd roundrect
			(at 4.75 -2.2)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GNSS_I2C_SDA")
		)
		(pad "17" smd roundrect
			(at 4.75 -3.3)
			(size 1.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GNSS_I2C_SCL")
		)
		(pad "18" smd roundrect
			(at 4.75 -4.4)
			(size 1.8 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/RF_GPS.3dshapes/ublox_MAX.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM03B-SRSS-TB_1x03-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 39 60.7)
		(descr "JST SH series connector, SM03B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)")
		(tags "connector JST SH horizontal")
		(property "Reference" "J2"
			(at 0 -3.98 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SM03B-SRSS-TB"
			(at 0 3.98 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/SMD_single_row_plus_mounting_pad"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(pad "2" smd roundrect
			(at 0 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/HOST_UART_TX")
		)
		(pad "3" smd roundrect
			(at 1 -2)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/HOST_UART_RX")
		)
		(pad "MP" smd roundrect
			(at -2.3 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
		)
		(pad "MP" smd roundrect
			(at 2.3 1.875)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM03B-SRSS-TB_1x03-1MP_P1.00mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Bourns_SRR1260"
		(layer "F.Cu")
		(at 70 47 180)
		(descr "Bourns SRR1260 series SMD inductor http://www.bourns.com/docs/Product-Datasheets/SRR1260.pdf")
		(tags "Bourns SRR1260 SMD inductor")
		(property "Reference" "L1"
			(at 0 -7.25 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1mH SRR1260"
			(at 0 7.4 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.85 0 180)
			(size 2.9 5.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/3V3")
		)
		(pad "2" smd rect
			(at 4.85 0 180)
			(size 2.9 5.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SW")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRR1260.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 55.5 42.6)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/3V3")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/GND")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 46 55.5)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP15"
			(at 0 -1.648 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GPIO_HV_PWM"
			(at 0 1.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net "/GPIO_HV_PWM")
		)
		(embedded_fonts no)
	)
	(footprint "GC1_RevD:XIAO_ESP32S3"
		(layer "F.Cu")
		(at 30.5 46)
		(property "Reference" "MOD1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Seeed XIAO ESP32S3"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd roundrect
			(at -7.62 7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net "/HV_SENSE")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -5.08 7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net "/GPIO_GM_COUNT")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at -2.54 7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at 0 7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net "/GPIO_HV_PWM")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 2.54 7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net "/GNSS_I2C_SDA")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 5.079999 7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net "/GNSS_I2C_SCL")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at 7.62 7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net "/HOST_UART_TX_RAW")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at 7.62 -7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net "/HOST_UART_RX_RAW")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd roundrect
			(at 5.08 -7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(thermal_bridge_angle 45)
		)
		(pad "10" smd roundrect
			(at 2.54 -7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(thermal_bridge_angle 45)
		)
		(pad "11" smd roundrect
			(at 0 -7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(thermal_bridge_angle 45)
		)
		(pad "12" smd roundrect
			(at -2.54 -7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net "/3V3")
			(thermal_bridge_angle 45)
		)
		(pad "13" smd roundrect
			(at -5.079999 -7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net "/GND")
			(thermal_bridge_angle 45)
		)
		(pad "14" smd roundrect
			(at -7.62 -7.62)
			(size 1.5 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net "/VBUS")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "GC1_RevD:Tube_Polarity_Links"
		(layer "B.Cu")
		(at 54.8 24)
		(property "Reference" "JP1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Tube polarity links"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd roundrect
			(at -2.5 -2.5)
			(size 1.2 1.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.2)
			(net "/TUBE_LEFT")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 2.5 -2.5)
			(size 1.2 1.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.2)
			(net "/GM_ANODE")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at -2.5 2.5)
			(size 1.2 1.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.2)
			(net "/GM_CATHODE")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at 2.5 2.5)
			(size 1.2 1.2)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.2)
			(net "/TUBE_RIGHT")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(gr_arc
		(start 20 22)
		(mid 20.585786 20.585786)
		(end 22 20)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20 62)
		(end 20 22)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 22 20)
		(end 84 20)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 22 64)
		(mid 20.585786 63.414213)
		(end 20 62)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 84 20)
		(mid 85.414213 20.585786)
		(end 86 22)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84 64)
		(end 22 64)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86 22)
		(end 86 62)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 86 62)
		(mid 85.414213 63.414213)
		(end 84 64)
		(layer "Edge.Cuts")
	)
	(gr_text "TP11"
		(at 22.5 57.5 0)
		(layer "F.SilkS")
	)
	(gr_text "TP12"
		(at 25.5 57.4 0)
		(layer "F.SilkS")
	)
	(gr_text "TP13"
		(at 28.5 61 0)
		(layer "F.SilkS")
	)
	(gr_text "UART 1:G 2:TX 3:RX"
		(at 28.5 62.7 0)
		(layer "F.SilkS")
	)
	(gr_text "TP9"
		(at 29 32.5 0)
		(layer "F.SilkS")
	)
	(gr_text "TP14"
		(at 32 57.4 0)
		(layer "F.SilkS")
	)
	(gr_text "TP10"
		(at 33 32.5 0)
		(layer "F.SilkS")
	)
	(gr_text "TP17"
		(at 44 39.2 0)
		(layer "F.SilkS")
	)
	(gr_text "TP7"
		(at 44 59.5 0)
		(layer "F.SilkS")
	)
	(gr_text "MC1"
		(at 45.5 28.5 0)
		(layer "F.SilkS")
	)
	(gr_text "TP4"
		(at 46 48.5 0)
		(layer "F.SilkS")
	)
	(gr_text "TP15"
		(at 46 54 0)
		(layer "F.SilkS")
	)
	(gr_text "TP3"
		(at 49 38.7 0)
		(layer "F.SilkS")
	)
	(gr_text "TP16"
		(at 50 57.2 0)
		(layer "F.SilkS")
	)
	(gr_text "TP2"
		(at 51.8 28.5 0)
		(layer "F.SilkS")
	)
	(gr_text "SBM-21"
		(at 54 20.8 0)
		(layer "F.SilkS")
	)
	(gr_text "TP6"
		(at 57 34.5 0)
		(layer "F.SilkS")
	)
	(gr_text "MC2"
		(at 65 28.5 0)
		(layer "F.SilkS")
	)
	(gr_text "TP5"
		(at 67 56.6 0)
		(layer "F.SilkS")
	)
	(gr_text "TP1"
		(at 70.1 27.2 0)
		(layer "F.SilkS")
	)
	(gr_text "HV DIVIDER"
		(at 71.5 36 0)
		(layer "F.SilkS")
	)
	(gr_text "TP8"
		(at 74.5 60.5 0)
		(layer "F.SilkS")
	)
	(gr_text "USB-C SERVICE / POWER"
		(at 20.9 47 90)
		(layer "F.SilkS")
	)
	(gr_text "HV BOOST"
		(at 82 47 90)
		(layer "F.SilkS")
	)
	(gr_text "DANGER: ~400 V HIGH VOLTAGE"
		(at 85.1 41.8 90)
		(layer "F.SilkS")
	)
	(gr_text "~400 VDC - DISCONNECT POWER"
		(at 31 24.7 0)
		(layer "B.SilkS")
	)
	(gr_text "GC1 REV D | GEIGER + GNSS"
		(at 32 21 0)
		(layer "B.SilkS")
	)
	(gr_text "1"
		(at 51.15 21.5 0)
		(layer "B.SilkS")
	)
	(gr_text "3"
		(at 51.15 26.5 0)
		(layer "B.SilkS")
	)
	(gr_text "POWER OFF / DISCONNECT USB BEFORE HANDLING."
		(at 53 30.2 0)
		(layer "B.SilkS")
	)
	(gr_text "HV-RATED METER: VERIFY TP8 BELOW 5 V BEFORE SERVICE."
		(at 53 31.6 0)
		(layer "B.SilkS")
	)
	(gr_text "DO NOT TOUCH HV, TUBE CONTACTS, OR COPPER WHILE ENERGIZED."
		(at 53 33.4 0)
		(layer "B.SilkS")
	)
	(gr_text "KEEP DRY; INSULATE FROM ENCLOSURE; NOT A CERTIFIED DOSIMETER."
		(at 53 35.7 0)
		(layer "B.SilkS")
	)
	(gr_text "1  SECURE USING ALL 3x M2 HOLES; DO NOT DEFEAT KEEPOUTS."
		(at 53 41.4 0)
		(layer "B.SilkS")
	)
	(gr_text "2  J2: 1 GND | 2 TX -> HOST RX | 3 RX <- HOST TX."
		(at 53 43.7 0)
		(layer "B.SilkS")
	)
	(gr_text "3  UART IS 3.3 V ONLY. NEVER APPLY 5 V TO J2."
		(at 53 46 0)
		(layer "B.SilkS")
	)
	(gr_text "4  VERIFY HOST PINOUT, POLARITY, AND COMMON GROUND FIRST."
		(at 53 48.3 0)
		(layer "B.SilkS")
	)
	(gr_text "5  KEEP HARNESS CLEAR OF HV PARTS, ANTENNA, AND WASHERS."
		(at 53 50.6 0)
		(layer "B.SilkS")
	)
	(gr_text "SERVICE: USB-C IS FOR POWER / PROGRAMMING."
		(at 53 54 0)
		(layer "B.SilkS")
	)
	(gr_text "RX ELECTRICAL PATH REQUIRES MATCHING GC1 FIRMWARE."
		(at 53 56.3 0)
		(layer "B.SilkS")
	)
	(gr_text "USE HV-RATED TOOLS AND EYE PROTECTION DURING BRING-UP."
		(at 53 58.6 0)
		(layer "B.SilkS")
	)
	(gr_text "ENGINEERING PROTOTYPE - VERIFY BEFORE USE."
		(at 53 62.3 0)
		(layer "B.SilkS")
	)
	(gr_text "JP1"
		(at 54.8 24 0)
		(layer "B.SilkS")
	)
	(gr_text "2"
		(at 58.449999 21.5 0)
		(layer "B.SilkS")
	)
	(gr_text "4"
		(at 58.449999 26.5 0)
		(layer "B.SilkS")
	)
	(gr_text "INSTALL:"
		(at 53 39.1 0)
		(layer "B.SilkS")
	)
	(zone
		(net "/GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 20.3 20.3) (xy 85.7 20.3) (xy 85.7 63.7) (xy 20.3 63.7)
			)
		)
	)
	(zone
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 88 60.5) (xy 87.973515 61.039094) (xy 87.894319 61.572996) (xy 87.763171 62.096565) (xy 87.581337 62.604758)
				(xy 87.350566 63.092682) (xy 87.073082 63.555636) (xy 86.751557 63.989163) (xy 86.389087 64.389087)
				(xy 85.989163 64.751557) (xy 85.555636 65.073082) (xy 85.092682 65.350566) (xy 84.604758 65.581337)
				(xy 84.096565 65.763171) (xy 83.572996 65.894319) (xy 83.039094 65.973515) (xy 82.5 66) (xy 81.960905 65.973515)
				(xy 81.427003 65.894319) (xy 80.903434 65.763171) (xy 80.395241 65.581337) (xy 79.907317 65.350566)
				(xy 79.444363 65.073082) (xy 79.010836 64.751557) (xy 78.610912 64.389087) (xy 78.248442 63.989163)
				(xy 77.926917 63.555636) (xy 77.649433 63.092682) (xy 77.418662 62.604758) (xy 77.236828 62.096565)
				(xy 77.10568 61.572996) (xy 77.026484 61.039094) (xy 77 60.5) (xy 77.026484 59.960905) (xy 77.10568 59.427003)
				(xy 77.236828 58.903434) (xy 77.418662 58.395241) (xy 77.649433 57.907317) (xy 77.926917 57.444363)
				(xy 78.248442 57.010836) (xy 78.610912 56.610912) (xy 79.010836 56.248442) (xy 79.444363 55.926917)
				(xy 79.907317 55.649433) (xy 80.395241 55.418662) (xy 80.903434 55.236828) (xy 81.427003 55.10568)
				(xy 81.960905 55.026484) (xy 82.5 55) (xy 83.039094 55.026484) (xy 83.572996 55.10568) (xy 84.096565 55.236828)
				(xy 84.604758 55.418662) (xy 85.092682 55.649433) (xy 85.555636 55.926917) (xy 85.989163 56.248442)
				(xy 86.389087 56.610912) (xy 86.751557 57.010836) (xy 87.073082 57.444363) (xy 87.350566 57.907317)
				(xy 87.581337 58.395241) (xy 87.763171 58.903434) (xy 87.894319 59.427003) (xy 87.973515 59.960905)
			)
		)
	)
	(zone
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 88 23.5) (xy 87.973515 24.039094) (xy 87.894319 24.572996) (xy 87.763171 25.096565) (xy 87.581337 25.604758)
				(xy 87.350566 26.092682) (xy 87.073082 26.555636) (xy 86.751557 26.989163) (xy 86.389087 27.389087)
				(xy 85.989163 27.751557) (xy 85.555636 28.073082) (xy 85.092682 28.350566) (xy 84.604758 28.581337)
				(xy 84.096565 28.763171) (xy 83.572996 28.894319) (xy 83.039094 28.973515) (xy 82.5 29) (xy 81.960905 28.973515)
				(xy 81.427003 28.894319) (xy 80.903434 28.763171) (xy 80.395241 28.581337) (xy 79.907317 28.350566)
				(xy 79.444363 28.073082) (xy 79.010836 27.751557) (xy 78.610912 27.389087) (xy 78.248442 26.989163)
				(xy 77.926917 26.555636) (xy 77.649433 26.092682) (xy 77.418662 25.604758) (xy 77.236828 25.096565)
				(xy 77.10568 24.572996) (xy 77.026484 24.039094) (xy 77 23.5) (xy 77.026484 22.960905) (xy 77.10568 22.427003)
				(xy 77.236828 21.903434) (xy 77.418662 21.395241) (xy 77.649433 20.907317) (xy 77.926917 20.444363)
				(xy 78.248442 20.010836) (xy 78.610912 19.610912) (xy 79.010836 19.248442) (xy 79.444363 18.926917)
				(xy 79.907317 18.649433) (xy 80.395241 18.418662) (xy 80.903434 18.236828) (xy 81.427003 18.10568)
				(xy 81.960905 18.026484) (xy 82.5 18) (xy 83.039094 18.026484) (xy 83.572996 18.10568) (xy 84.096565 18.236828)
				(xy 84.604758 18.418662) (xy 85.092682 18.649433) (xy 85.555636 18.926917) (xy 85.989163 19.248442)
				(xy 86.389087 19.610912) (xy 86.751557 20.010836) (xy 87.073082 20.444363) (xy 87.350566 20.907317)
				(xy 87.581337 21.395241) (xy 87.763171 21.903434) (xy 87.894319 22.427003) (xy 87.973515 22.960905)
			)
		)
	)
	(zone
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 51.2 60.5) (xy 51.184591 60.813654) (xy 51.138512 61.124289) (xy 51.062209 61.42891) (xy 50.956414 61.724586)
				(xy 50.822148 62.008469) (xy 50.660702 62.277824) (xy 50.473633 62.530058) (xy 50.262741 62.762741)
				(xy 50.030058 62.973633) (xy 49.777824 63.160702) (xy 49.508469 63.322148) (xy 49.224586 63.456414)
				(xy 48.92891 63.562209) (xy 48.624289 63.638512) (xy 48.313654 63.684591) (xy 48 63.7) (xy 47.686345 63.684591)
				(xy 47.37571 63.638512) (xy 47.071089 63.562209) (xy 46.775413 63.456414) (xy 46.49153 63.322148)
				(xy 46.222175 63.160702) (xy 45.969941 62.973633) (xy 45.737258 62.762741) (xy 45.526366 62.530058)
				(xy 45.339297 62.277824) (xy 45.177851 62.008469) (xy 45.043585 61.724586) (xy 44.93779 61.42891)
				(xy 44.861487 61.124289) (xy 44.815408 60.813654) (xy 44.8 60.5) (xy 44.815408 60.186345) (xy 44.861487 59.87571)
				(xy 44.93779 59.571089) (xy 45.043585 59.275413) (xy 45.177851 58.99153) (xy 45.339297 58.722175)
				(xy 45.526366 58.469941) (xy 45.737258 58.237258) (xy 45.969941 58.026366) (xy 46.222175 57.839297)
				(xy 46.49153 57.677851) (xy 46.775413 57.543585) (xy 47.071089 57.43779) (xy 47.37571 57.361487)
				(xy 47.686345 57.315408) (xy 48 57.3) (xy 48.313654 57.315408) (xy 48.624289 57.361487) (xy 48.92891 57.43779)
				(xy 49.224586 57.543585) (xy 49.508469 57.677851) (xy 49.777824 57.839297) (xy 50.030058 58.026366)
				(xy 50.262741 58.237258) (xy 50.473633 58.469941) (xy 50.660702 58.722175) (xy 50.822148 58.99153)
				(xy 50.956414 59.275413) (xy 51.062209 59.571089) (xy 51.138512 59.87571) (xy 51.184591 60.186345)
			)
		)
	)
	(zone
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 41 20.3) (xy 68 20.3) (xy 68 28.5) (xy 41 28.5)
			)
		)
	)
	(zone
		(net "/GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.2)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 20.3 20.3) (xy 85.7 20.3) (xy 85.7 63.7) (xy 20.3 63.7)
			)
		)
	)
	(zone
		(net "/GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 20.3 20.3) (xy 54 20.3) (xy 54 63.7) (xy 20.3 63.7)
			)
		)
	)
	(zone
		(net "/GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 20.3 20.3) (xy 54 20.3) (xy 54 63.7) (xy 20.3 63.7)
			)
		)
	)
	(embedded_fonts no)
)
